Title of the Abstract

Ivanov I.I.1), Serov V.V. 2)
1) Kutateladze Institute of Thermophysics, Siberian Branch of the RAS, Novosibirsk, Russia
2) Novosibirsk State University, Novosibirsk, Russia 

The liquid passes into a metastable state with a rapid decrease in pressure in the liquid to levels below the saturation pressure [1].

		(1)

In fig. 1 shows the calculated conversion curve and the corresponding experimental points.

Fig. 1. Dependence of the final conversion on the contact time.

To test the model, numerical calculations were compared with experimental results (Table 1).

Table 1. Comparison of experimental data with calculated values

Namt	Experimental value	Calculated value	
Pressure, Pa	26	25,9	

References

1.	Labuntsov D.A. Modern concepts of the mechanism of nucleate boiling in a liquid - Moscow: Nauka, 1974.  – 150 p.
2.	4.	Bradfield W.S. Solid-liquid contact in stable film boiling // Ind. Eng. Chem. Fundam. – 1966. –
V. 5. – P. 200–204.
3.	Reference book on thermohydraulic calculations / Kirillov P.L., Yuriev Yu.S., Bobkov V.P.; ed. Kirillova P.L. - M: Energoatomizdat, 1990. –358 p.
4.	Litvintsev K.Yu., Amelchugov S.P., Dekterev A.A. Modeling the development of a fire based on the software complex "SigmaFire" // Book of abstracts XIV Int. conf. on the problems of fire safety. - Moscow, 2012. - V. 1. - P. 89-91.